6200, 6201, 6203, 6208, 6209, 6210, 6220, 6215, 6225, 6218,
6228, 6260, 6265,
ST6200, ST6201:
INT: NMI=6, PORTA=1, PORTB=2, TIMER=3, ADC=4,
PINS: PA1=15, PA2=14, PA3=13,
	PB0=12, PB1=11, PB3=10, PB5=09, PB6=08, PB7=07,
	RESET=06, NMI=04,
	TEST=05, OSCIN=02, OSCOUT=03, VDD=01, VSS=16,
.ADC: PB3, PB5, PB6, PB7,
*16
ST6203:
INT: NMI=6, PORTA=1, PORTB=2, TIMER=3,
PINS: PA1=15, PA2=14, PA313,
	PB0=12, PB1=11, PB3=10, PB5=09, PB6=08, PB7=07,
	RESET=06, NMI=04,
	TEST=05, OSCIN=02, OSCOUT=03, VDD=01, VSS=16,
*16
ST6208:
INT: NMI=6, PORTA=1, PORTB=2, TIMER=3,
PINS: PA0=19,PA1=18, PA2=17, PA3=16,
	PB0=15, PB1=14, PB2=13, PB3=12, PB4=11, PB5=10, PB6=09, PB7=08,
	RESET=07, NMI=05, TIMER=02,
	TEST=06, OSCIN=03, OSCOUT=04, VDD=01, VSS=20,
*20
ST6209:
INT: NMI=6, PORTA=1, PORTB=2, TIMER=3,
PINS: PA0=19,PA1=18, PA2=17, PA3=16,
	PB0=15, PB1=14, PB2=13, PB3=12, PB4=11, PB5=10, PB6=09, PB7=08,
	RESET=07, NMI=05, TIMER=02,
	TEST=06, OSCIN=03, OSCOUT=04, VDD=01, VSS=20,
.ADC : PB4, PB5, PB6, PB7,
*20
ST6210, ST6211, ST6213, ST6214, ST6220, ST6221, ST6223, ST6224:
INT: NMI=6, PORTA=1, PORTB=2, TIMER=3, ADC=4,
PINS: PA0=19, PA1=18, PA2=17, PA3=16,
	PB0=15, PB1=14, PB2=13, PB3=12, PB4=11, PB5=10, PB6=09, PB7=08,
	RESET=07, NMI=05, TIMER=02,
	TEST=06, OSCIN=03, OSCOUT=04, VDD=01, VSS=20,
.ADC: PB0, PB1, PB2, PB3, PB4, PB5, PB6, PB7,
*20
ST6215, ST6216, ST6225:
INT: NMI=6, PORTA=1, PORTB=2, PORTC=2, TIMER=3, ADC=4,
PINS: PA0=27, PA1=26, PA2=25, PA3=24, PA4=23, PA5=22, PA6=21, PA7=20,
	PB0=19, PB1=18, PB2=17, PB3=16, PB4=15, PB5=14, PB6=13, PB7=12,
	PC4=09, PC5=08, PC6=07, PC7=06,
	RESET=11, NMI=05, TIMER=02,
	TEST=10, OSCIN=03, OSCOUT=04, VDD=01, VSS=28,
.ADC: PA4, PA5, PA6, PA7,
	PB0, PB1, PB2, PB3, PB4, PB5, PB6, PB7,
	PC4, PC5, PC6, PC7,
*28
ST6218:
INT: NMI=6, PORTA=1, PORTB=2, PORTD=2, TIMER=4, ADC=4, ARTIMER=3, UART=4,
PINS: PA1=19, PA2=18, PA3=17, PA4=16, PA5=15,
	PB4=10, PB5=09, PB6=08,
	PD4=14, PD5=13, PD6=12, PD7=11,
	RESET=07, NMI=05, TIMER=02,
	TEST=06, OSCIN=03, OSCOUT=04, VDD=01,VSS=20,
.ADC: PB4, PB5, PB6,
	PC4, PC5,
	PD4, PD5, PD6, PD7,
ARTIMIN=PA3, ARTIMOUT=PA2,
UARTRX=PD4, UARTTX=PD5,
*20
ST6228:
INT: NMI=6, PORTC=6, SPI=1, PORTA=1, PORTB=2, PORTD=2, ARTIMER=3, TIMER=4, UART=4, ADC=4,
PINS: PA0=27, PA1=26, PA2=25, PA3=24, PA4=23, PA5=22,
	PB4=14, PB5=13, PB6=12,
	PC4=09, PC5=08, PC6=07, PC7=06,
	PD1=21, PD2=20, PD3=19, PD4=18, PD5=17, PD6=16, PD7=15,
	RESET=11, NMI=05, TIMER=02,
	TEST=10, OSCIN=03, OSCOUT=04, VDD=01,VSS=28,
.ADC: PB4, PB5, PB6,
	PC4, PC5,
	PD1, PD2, PD3, PD4, PD5, PD6, PD7,
ARTIMIN=PA3, ARTIMOUT=PA2,
SPIIN=PD2, SPIOUT=PD3, SPICLK=PD1,
UARTRX=PD4, UARTTX=PD5,
*28
ST6230:
INT: NMI=6, PORTC=0, PORTA=1, PORTB=2, PORTD=2, TIMER16=3, TIMER=4, UART=4, ADC=4,
PINS: PA0, PA1, PA2, PA3, PA4, PA5,
	PB4, PB5, PB6,
	PC4, PC5, PC6, PC7,
	PD1, PD2, PD3, PD4, PD5, PD6, PD7,
	RESET, NMI, TIMER, TIMER1,
*
ST6232:
INT: NMI=6, PORTC=0, PORTA=1, PORTB=2, PORTD=2, TIMER16=3, TIMER=4, UART=4, ADC=4,
PINS: PA0, PA1, PA2, PA3, PA4, PA5, PA6, PA7,
	PB0, PB3, PB4, PB5, PB6, PB7,
	PC5, PC6, PC7,
	PD0, PD1, PD2, PD3, PD4, PD5, PD6, PD7,
	RESET, NMI, TIMER, TIMER1,
*
ST6235:
INT: NMI=6, PORTC=0, PORTA=1, PORTB=2, PORTD=2, TIMER16=3, TIMER=4, UART=4, ADC=4,
PINS: PA0, PA1, PA2, PA3, PA4, PA5, PA6, PA7,
	PB0, PB1, PB2, PB3, PB4, PB5, PB6, PB7,
	PC4, PC5, PC6, PC7,
	PD0, PD1, PD2, PD3, PD4, PD5, PD6, PD7,
	RESET, NMI, TIMER, TIMER1,
*
ST6231:
INT: NMI=6, PORTA=1, PORTB=2, TIMER=3, ADC=4,
PINS: PA0, PA1, PA2, PA3, PA4, PA5, PA6, PA7,
	PB0, PB1, PB2, PB3, PB4, PB5, PB6, PB7,
	RESET, NMI, TIMER1, TIMER2,
*
ST6242:
INT: NMI=6, SPI=1, PORTA=2, PORTB=2, TIMER=3, ADC=4,
PINS:  PA4, PA5, PA6, PA7,
	PB2, PB3, PB4, PB5, PB6, PB7,
	RESET, NMI, TIMER,
*
ST6240, ST6243, ST6244:
INT: NMI=6, SPI=1, PORTA=2, PORTB=2, TIMER=3, TIMER1=3, TIMER2=3, ADC=4,
PINS: PA0, PA1, PA2, PA3, PA4, PA5, PA6, PA7,
	PB0, PB1, PB2, PB3, PB4, PB5, PB6, PB7,
	RESET, NMI, TIMER,
*
ST6245:
INT: NMI=6, SPI=1, PORTA=2, PORTB=2, TIMER=3, TIMER1=3, TIMER2=3, ADC=4,
PINS: PA5, PA6, PA7,
	PB0, PB1, PB2, PB3, PB4, PB5, PB6, PB7,
	RESET, NMI, TIMER,
*
ST6291, ST6293:
INT: NMI=6, PORTA=1, PORTB=1, PORTC=2, TIMER=3, ADC=4,
PINS: PA0, PA1, PA2, PA3,
	PB0, PB1, PB2, PB3, PB6, PB7,
	PC2, PC3, PC4,
	RESET, NMI, TIMER,
*
ST6292, ST6294:
INT: NMI=6, PORTA=1, PORTB=1, PORTC=2, TIMER=3, ADC=4,
PINS:  PA0, PA1, PA2, PA3, PA4, PA5, PA6, PA7,
	PB0, PB1, PB2, PB3, PB4, PB5, PB6, PB7,
	PC0, PC1, PC2, PC3, PC4,
	RESET, NMI, TIMER,
*
ST6253:
INT: NMI=6, PORTA=1, PORTB=1, PORTC=2, ARTIMER=3, ADC=4, TIMER=4,
PINS: PA0=08, PA1=11, PA2=12, PA3=13,
	PB0=01, PB1=02, PB2=04, PB3=05, PB6=06, PB7=07,
	PC2=20, PC3=19, PC4=18,
	RESET=16, NMI=17,
	TEST=03, OSCIN=14, OSCOUT=15, VDD=09,VSS=10,
.ADC: PA0, PA1, PA2, PA3, PC2, PC3, PC4,
ARTIMIN=PB6, ARTIMOUT=PB7,
*20
ST6260:
INT: NMI=6, PORTA=1, PORTB=1, SPI=2, PORTC=2, ARTIMER=3, ADC=4, TIMER=4,
PINS: PA0=08, PA1=11, PA2=12, PA3=13,
	PB0=01, PB1=02, PB2=04, PB3=05, PB6=06, PB7=07,
	PC2=20, PC3=19, PC4=18,
	RESET=16, NMI=17,
	TEST=03, OSCIN=14, OSCOUT=15, VDD=09,VSS=10,
.ADC: PA0, PA1, PA2, PA3, PC2, PC3, PC4,
ARTIMIN=PB6, ARTIMOUT=PB7,
SPIIN=PC2, SPIOUT=PC3, SPICLK=PC4,   
*20
ST6263:
INT: NMI=6, PORTA=1, PORTB=1, PORTC=2, ARTIMER=3, ADC=4, TIMER=4,
PINS: PA0=08, PA1=11, PA2=12, PA3=13,
	PB0=01, PB1=02, PB2=04, PB3=05, PB6=06, PB7=07,
	PC2=20, PC3=19, PC4=18,
	RESET=16, NMI=17,
	TEST=03, OSCIN=14, OSCOUT=15, VDD=09,VSS=10,
.ADC: PA0, PA1, PA2, PA3, PC2, PC3, PC4,
ARTIMIN=PB6, ARTIMOUT=PB7,  
*20
ST6265:
INT: NMI=6, SPI=2, PORTA=1, PORTB=1, PORTC=2, ARTIMER=3, ADC=4, TIMER=4,
PINS: PA0=10, PA1=13, PA2=14, PA3=15, PA4=16, PA5=17, PA6=18, PA7=19,
	PB0=01, PB1=02, PB2=04, PB3=05, PB4=06, PB5=07, PB6=08, PB7=09,
	PC0=28, PC1=27, PC2=26, PC3=25, PC4=24,
	RESET=22, NMI=23,
	TEST=03, OSCIN=20, OSCOUT=21, VDD=11,VSS=12,
.ADC: PA0, PA1, PA2, PA3, PA4, PA5,PA6, PA7, PC0, PC1, PC2, PC3, PC4,
ARTIMIN=PB6, ARTIMOUT=PB7,
SPIIN=PC2, SPIOUT=PC3, SPICLK=PC4,
TIM=PC1
*28
ST6280:
INT: NMI=6, SPI=1, PORTA=2, PORTB=2, PORTC=2, TIMER=3, ADC=4,
PINS:  PA2, PA3, PA4, PA5, PA6, PA7,
	PB0, PB1, PB2, PB3, PB4, PB5, PB6, PB7,
	PC0, PC1, PC2, PC3, PC4, PC5, PC6, PC7,
	RESET, NMI, TIMER,
ARTIMIN=PB6, ARTIMOUT=PB7,
*
ST6285:
INT: NMI=6, SPI=1, PORTA=2, PORTB=2, PORTC=2, TIMER=3, ADC=4,
PINS:  PA4, PA5, PA6, PA7,
	PB0, PB1, PB2, PB3,
	PC4, PC5, PC6, PC7,
	RESET, NMI, TIMER,
ARTIMIN=PB6, ARTIMOUT=PB7,
*
ARTIMIN=PB6, ARTIMOUT=PB7,
*
